|  |  |  |
| --- | --- | --- |
| **EXIT SWITCH** | **PAUSE SWITCH** | **WIRE CONTROL** |
|  |  |  |
|  | Pause | Wire always heated |
| Long hold to  exit program and turn off Pi |  |  |
|  | Running | Wire controlled by program |